Registers Summary First Cut

Autogenerated register summary from file **Standards/register\_summary\_1.3.txt. Generated** 2020-04-29 23:42:48

Note that registers are defined using big endian notation. Bit 0 is the most significant bit!

# Block: 0x0001 : 1x/4x LP-Serial Register Block

|  |  |  |  |
| --- | --- | --- | --- |
| Name: 1x/4x LP-Serial Register Block Header Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | EF\_PTR | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| 16:31 | EF\_ID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| Name: Port Link Time-out Control CSR Offset: 0x20 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.2 Port Link Time-out Control CSR (Block Offset 0x20) |
| 24:31 | Reserved | | |
| Name: Port Response Time-out Control CSR Offset: 0x24 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.3 Port Response Time-out Control CSR (Block Offset 0x24) |
| 24:31 | Reserved | | |
| Name: Port General Control CSR Offset: 0x3C | | | |
| Bits | Name | Part | Section |
| 0 | Host | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.4 Port General Control CSR (Block Offset 0x3C) |
| 1 | Master Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.4 Port General Control CSR (Block Offset 0x3C) |
| 2 | Discovered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.4 Port General Control CSR (Block Offset 0x3C) |
| 3:31 | Reserved | | |
| Name: Port n Error and Status CSRs Offset: 0x58, 78, ..., 238 | | | |
| Bits | Name | Part | Section |
| 0:4 | Reserved | | |
| 5 | Output Packet-dropped | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, ..., 238) |
| 6 | Output Failed-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, ..., 238) |
| 7 | Output Degraded-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, ..., 238) |
| 8:10 | Reserved | | |
| 11 | Output Retry-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 12 | Output Retried | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 13 | Output Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 14 | Output Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 15 | Output Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 16:20 | Reserved | | |
| 21 | Input Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 22 | Input Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 23 | Input Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 24:26 | Reserved | | |
| 27 | Port-write Pending | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 28 | Reserved | | |
| 29 | Port Error | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 30 | Port OK | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| 31 | Port Uninitialized | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.5 Port n Error and Status CSRs (Block Offsets 0x58, 78, ..., 238) |
| Name: Port n Control CSR Offset: 0x5C, 7C, ..., 23C | | | |
| Bits | Name | Part | Section |
| 0:1 | Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 2:4 | Initialized Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 5:7 | Port Width Override | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 8 | Port Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 9 | Output Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 10 | Input Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 11 | Error Checking Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 12 | Multicast-event Participant | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 13 | Flow Control Participant | RapidIO Interconnect Specification Part 9: Flow Control Logical Layer Extensions Specification | 4.3 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 14 | Enumeration Boundary | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 15:19 | Reserved | | |
| 20:27 | Re-transmit Suppression Mask | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 28 | Stop on Port Failed-encountered Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 29 | Drop Packet Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 30 | Port Lockout | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 31 | Port Type | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.5.2.6 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |

# Block: 0x0002 : 1x/4x LP-Serial Register Block

|  |  |  |  |
| --- | --- | --- | --- |
| Name: 1x/4x LP-Serial Register Block Header Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | EF\_PTR | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| 16:31 | EF\_ID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| Name: Port Link Time-out Control CSR Offset: 0x20 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.2 Port Link Time-out Control CSR (Block Offset 0x20) |
| 24:31 | Reserved | | |
| Name: Port Response Time-out Control CSR Offset: 0x24 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.3 Port Response Time-out Control CSR (Block Offset 0x24) |
| 24:31 | Reserved | | |
| Name: Port General Control CSR Offset: 0x3C | | | |
| Bits | Name | Part | Section |
| 0 | Host | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.4 Port General Control CSR (Block Offset 0x3C) |
| 1 | Master Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.4 Port General Control CSR (Block Offset 0x3C) |
| 2 | Discovered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.4 Port General Control CSR (Block Offset 0x3C) |
| 3:31 | Reserved | | |
| Name: Port n Link Maintenance Request CSRs Offset: 0x40, 60, ..., 220 | | | |
| Bits | Name | Part | Section |
| 0:28 | Reserved | | |
| 29:31 | Command | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.5 Port n Link Maintenance Request CSRs (Block Offsets 0x40, 60, ..., 220) |
| Name: Port n Link Maintenance Response CSRs Offset: 0x44, 64, ..., 224 | | | |
| Bits | Name | Part | Section |
| 0 | response\_valid | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.6 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| 1:21 | Reserved | | |
| 22:26 | ackID\_status | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.6 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| 27:31 | link\_status | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.6 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| Name: Port n Local ackID CSRs Offset: 0x48, 68, ..., 228 | | | |
| Bits | Name | Part | Section |
| 0 | Clr\_outstanding\_ackIDs | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.7 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 1:2 | Reserved | | |
| 3:7 | Inbound\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.7 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 8:18 | Reserved | | |
| 19:23 | Outstanding\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.7 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 24:26 | Reserved | | |
| 27:31 | Outbound\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.7 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| Name: Port n Error and Status CSRs Offset: 0x58, 78, ..., 238 | | | |
| Bits | Name | Part | Section |
| 0:4 | Reserved | | |
| 5 | Output Packet-dropped | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 6 | Output Failed-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 7 | Output Degraded-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 8:10 | Reserved | | |
| 11 | Output Retry-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 12 | Output Retried | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 13 | Output Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 14 | Output Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 15 | Output Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 16:20 | Reserved | | |
| 21 | Input Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 22 | Input Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 23 | Input Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 24:26 | Reserved | | |
| 27 | Port-write Pending | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 28 | Reserved | | |
| 29 | Port Error | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 30 | Port OK | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 31 | Port Uninitialized | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.8 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| Name: Port n Control CSR Offset: 0x5C, 7C, ..., 23C | | | |
| Bits | Name | Part | Section |
| 0:1 | Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 2:4 | Initialized Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 5:7 | Port Width Override | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 8 | Port Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 9 | Output Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 10 | Input Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 11 | Error Checking Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 12 | Multicast-event Participant | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 13 | Flow Control Participant | RapidIO Interconnect Specification Part 9: Flow Control Logical Layer Extensions Specification | 4.3 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 14 | Enumeration Boundary | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 15:19 | Reserved | | |
| 20:27 | Re-transmit Suppression Mask | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 28 | Stop on Port Failed-encountered Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 29 | Drop Packet Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 30 | Port Lockout | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 31 | Port Type | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.6.2.9 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |

# Block: 0x0003 : 1x/4x LP-Serial Register Block

|  |  |  |  |
| --- | --- | --- | --- |
| Name: 1x/4x LP-Serial Register Block Header Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | EF\_PTR | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| 16:31 | EF\_ID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| Name: Port Link Time-out Control CSR Offset: 0x20 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.2 Port Link Time-out Control CSR (Block Offset 0x20) |
| 24:31 | Reserved | | |
| Name: Port General Control CSR Offset: 0x3C | | | |
| Bits | Name | Part | Section |
| 0:1 | Reserved | | |
| 2 | Discovered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.3 Port General Control CSR (Block Offset 0x3C) |
| 3:31 | Reserved | | |
| Name: Port n Error and Status CSRs Offset: 0x58, 78, .., 238 | | | |
| Bits | Name | Part | Section |
| 0:4 | Reserved | | |
| 5 | Output Packet-dropped | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, .., 238) |
| 6 | Output Failed-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, .., 238) |
| 7 | Output Degraded-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x58, 78, .., 238) |
| 8:10 | Reserved | | |
| 11 | Output Retry-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 12 | Output Retried | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 13 | Output Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 14 | Output Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 15 | Output Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 16:20 | Reserved | | |
| 21 | Input Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 22 | Input Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 23 | Input Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 24:26 | Reserved | | |
| 27 | Port-write Pending | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 28 | Reserved | | |
| 29 | Port Error | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 30 | Port OK | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| 31 | Port Uninitialized | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.4 Port n Error and Status CSRs (Block Offsets 0x58, 78, .., 238) |
| Name: Port n Control CSR Offset: 0x5C, 7C, ..., 23C | | | |
| Bits | Name | Part | Section |
| 0:1 | Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 2:4 | Initialized Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 5:7 | Port Width Override | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 8 | Port Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 9 | Output Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 10 | Input Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 11 | Error Checking Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 12 | Multicast Event Participant | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 13 | Flow Control Participant | RapidIO Interconnect Specification Part 9: Flow Control Logical Layer Extensions Specification | 4.3 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 14 | Enumeration Boundary | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 15:19 | Reserved | | |
| 20:27 | Re-transmit Suppression Mask | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 28 | Stop on Port Failed-encountered Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 29 | Drop Packet Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 30 | Port Lockout | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 31 | Port Type | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.7.2.5 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |

# Block: 0x0007 : Error Management Extensions Block

|  |  |  |  |
| --- | --- | --- | --- |
| Name: Error Management Extensions Block Header Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | EF\_PTR | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.1 Error Management Extensions Block Header (Block Offset 0x0) |
| 16:31 | EF\_ID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.1 Error Management Extensions Block Header (Block Offset 0x0) |
| Name: Logical/Transport Layer Error Detect CSR Offset: 0x08 | | | |
| Bits | Name | Part | Section |
| 0 | IO error response | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 1 | Message error response | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 2 | GSM error response | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 3 | Message Format Error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 4 | Illegal transaction decode | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 5 | Illegal transaction target error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 6 | Message Request Time-out | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 7 | Packet Response Time-out | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 8 | Unsolicited Response | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 9 | Unsupported Transaction | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| 10:23 | Reserved | | |
| 24:31 | Implementation Specific error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.2 Logical/Transport Layer Error Detect CSR (Block Offset 0x08) |
| Name: Logical/Transport Layer Error Enable CSR Offset: 0x0C | | | |
| Bits | Name | Part | Section |
| 0 | IO error response enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 1 | Message error response enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 2 | GSM error response enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 3 | Message Format Error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 4 | Illegal transaction decode enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 5 | Illegal transaction target error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 6 | Message Request time-out enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 7 | Packet Response Time-out error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 8 | Unsolicited Response error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 9 | Unsupported Transaction error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| 10:23 | Reserved | | |
| 24:31 | Implementation Specific error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.3 Logical/Transport Layer Error Enable CSR (Block Offset 0x0C) |
| Name: Logical/Transport Layer High Address Capture CSR Offset: 0x10 | | | |
| Bits | Name | Part | Section |
| 0:31 | address[0-31] | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.4 Logical/Transport Layer High Address Capture CSR (Block Offset 0x10) |
| Name: Logical/Transport Layer Address Capture CSR Offset: 0x14 | | | |
| Bits | Name | Part | Section |
| 0:28 | address[32-60] | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.5 Logical/Transport Layer Address Capture CSR (Block Offset 0x14) |
| 29 | Reserved | | |
| 30:31 | xamsbs | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.5 Logical/Transport Layer Address Capture CSR (Block Offset 0x14) |
| Name: Logical/Transport Layer Device ID Capture CSR Offset: 0x18 | | | |
| Bits | Name | Part | Section |
| 0:7 | MSB destinationID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.6 Logical/Transport Layer Device ID Capture CSR (Block Offset 0x18) |
| 8:15 | destinationID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.6 Logical/Transport Layer Device ID Capture CSR (Block Offset 0x18) |
| 16:23 | MSB sourceID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.6 Logical/Transport Layer Device ID Capture CSR (Block Offset 0x18) |
| 24:31 | sourceID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.6 Logical/Transport Layer Device ID Capture CSR (Block Offset 0x18) |
| Name: Logical/Transport Layer Control Capture CSR Offset: 0x1C | | | |
| Bits | Name | Part | Section |
| 0:3 | ftype | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.7 Logical/Transport Layer Control Capture CSR (Block Offset 0x1C) |
| 4:7 | ttype | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.7 Logical/Transport Layer Control Capture CSR (Block Offset 0x1C) |
| 8:15 | msg info | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.7 Logical/Transport Layer Control Capture CSR (Block Offset 0x1C) |
| 16:31 | Implementation specific | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.7 Logical/Transport Layer Control Capture CSR (Block Offset 0x1C) |
| Name: Port-write Target deviceID CSR Offset: 0x28 | | | |
| Bits | Name | Part | Section |
| 0:7 | deviceID\_msb | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.8 Port-write Target deviceID CSR (Block Offset 0x28) |
| 8:15 | deviceID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.8 Port-write Target deviceID CSR (Block Offset 0x28) |
| 16 | large\_transport | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.8 Port-write Target deviceID CSR (Block Offset 0x28) |
| 17:31 | Reserved | | |
| Name: Packet Time-to-live CSR Offset: 0x2C | | | |
| Bits | Name | Part | Section |
| 0:15 | Time-to-live value | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.9 Packet Time-to-live CSR (Block Offset 0x2C) |
| 16:31 | Reserved | | |
| Name: Port n Error Detect CSR Offset: 0x40, 80,..., 400 | | | |
| Bits | Name | Part | Section |
| 0 | Implementation specific error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 1:7 | Reserved | | |
| 8 | Received S-bit error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 9 | Received corrupt control symbol | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 10 | Received acknowledge control symbol with unexpected ackID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 11 | Received packet-not-accepted control symbol | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 12 | Received packet with unexpected ackID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 13 | Received packet with bad CRC | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 14 | Received packet exceeds 276 Bytes | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 15:25 | Reserved | | |
| 26 | Non-outstanding ackID | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 27 | Protocol error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 28 | Frame toggle edge error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 29 | Delineation error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 30 | Unsolicited acknowledge control symbol | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| 31 | Link time-out | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.10 Port n Error Detect CSR (Block Offset 0x40, 80,..., 400) |
| Name: Port n Error Rate Enable CSR Offset: 0x44, 84,..., 404 | | | |
| Bits | Name | Part | Section |
| 0 | Implementation specific error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 1:7 | Reserved | | |
| 8 | Received S-bit error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 9 | Received control symbol with bad CRC enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 10 | Received out-of-sequence acknowledge control symbol enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 11 | Received packet-not-accepted control symbol enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 12 | Received packet with unexpected ackID enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 13 | Received packet with Bad CRC enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 14 | Received packet exceeds 276 Bytes enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 15:25 | Reserved | | |
| 26 | Non-outstanding ackID enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 27 | Protocol error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 28 | Frame toggle edge error enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 29 | Delineation error | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 30 | Unsolicited acknowledge control symbol | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| 31 | Link time-out | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.11 Port n Error Rate Enable CSR (Block Offset 0x44, 84,..., 404) |
| Name: Port n Attributes Capture CSR Offset: 0x48, 88,..., 408 | | | |
| Bits | Name | Part | Section |
| 0:1 | Info type | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.12 Port n Attributes Capture CSR (Block Offset 0x48, 88,..., 408) |
| 2 | Reserved | | |
| 3:7 | Error type | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.12 Port n Attributes Capture CSR (Block Offset 0x48, 88,..., 408) |
| 8:27 | Implementation Dependent | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.12 Port n Attributes Capture CSR (Block Offset 0x48, 88,..., 408) |
| 28:30 | Reserved | | |
| 31 | Capture valid info | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.12 Port n Attributes Capture CSR (Block Offset 0x48, 88,..., 408) |
| Name: Port n Packet/Control Symbol Capture 0 CSR Offset: 0x4C, 8C,..., 40C | | | |
| Bits | Name | Part | Section |
| 0:31 | Capture 0 | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.13 Port n Packet/Control Symbol Capture 0 CSR (Block Offset 0x4C, 8C,..., 40C) |
| Name: Port n Packet Capture 1 CSR Offset: 0x50, 90,..., 410 | | | |
| Bits | Name | Part | Section |
| 0:31 | Capture 1 | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.14 Port n Packet Capture 1 CSR (Block Offset 0x50, 90,..., 410) |
| Name: Port n Packet Capture 2 CSR Offset: 0x54, 94,..., 414 | | | |
| Bits | Name | Part | Section |
| 0:31 | Capture 2 | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.15 Port n Packet Capture 2 CSR (Block Offset 0x54, 94,..., 414) |
| Name: Port n Packet Capture 3 CSR Offset: 0x58, 98,..., 418 | | | |
| Bits | Name | Part | Section |
| 0:31 | Capture 3 | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.16 Port n Packet Capture 3 CSR (Block Offset 0x58, 98,..., 418) |
| Name: Port n Error Rate CSR Offset: 0x68, A8,..., 428 | | | |
| Bits | Name | Part | Section |
| 0:7 | Error Rate Bias | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.17 Port n Error Rate CSR (Block Offset 0x68, A8,..., 428) |
| 8:13 | Reserved | | |
| 14:15 | Error Rate Recovery | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.17 Port n Error Rate CSR (Block Offset 0x68, A8,..., 428) |
| 16:23 | Peak Error Rate | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.17 Port n Error Rate CSR (Block Offset 0x68, A8,..., 428) |
| 24:31 | Error Rate Counter | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.17 Port n Error Rate CSR (Block Offset 0x68, A8,..., 428) |
| Name: Port n Error Rate Threshold CSR Offset: 0x6C, AC,..., 42C | | | |
| Bits | Name | Part | Section |
| 0:7 | Error Rate Failed Threshold Trigger | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.18 Port n Error Rate Threshold CSR (Block Offset 0x6C, AC,..., 42C) |
| 8:15 | Error Rate Degraded Threshold Trigger | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.3.2.18 Port n Error Rate Threshold CSR (Block Offset 0x6C, AC,..., 42C) |
| 16:31 | Reserved | | |

# Block: 0x0009 : 1x/4x LP-Serial Register Block

|  |  |  |  |
| --- | --- | --- | --- |
| Name: 1x/4x LP-Serial Register Block Header Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | EF\_PTR | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| 16:31 | EF\_ID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.1 1x/4x LP-Serial Register Block Header (Block Offset 0x0) |
| Name: Port Link Time-out Control CSR Offset: 0x20 | | | |
| Bits | Name | Part | Section |
| 0:23 | time-out value | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.2 Port Link Time-out Control CSR (Block Offset 0x20) |
| 24:31 | Reserved | | |
| Name: Port General Control CSR Offset: 0x3C | | | |
| Bits | Name | Part | Section |
| 0:1 | Reserved | | |
| 2 | Discovered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.3 Port General Control CSR (Block Offset 0x3C) |
| 3:31 | Reserved | | |
| Name: Port n Link Maintenance Request CSRs Offset: 0x40, 60, ..., 220 | | | |
| Bits | Name | Part | Section |
| 0:28 | Reserved | | |
| 29:31 | Command | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.4 Port n Link Maintenance Request CSRs (Block Offsets 0x40, 60, ..., 220) |
| Name: Port n Link Maintenance Response CSRs Offset: 0x44, 64, ..., 224 | | | |
| Bits | Name | Part | Section |
| 0 | response\_valid | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.5 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| 1:21 | Reserved | | |
| 22:26 | ackID\_status | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.5 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| 27:31 | link\_status | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.5 Port n Link Maintenance Response CSRs (Block Offsets 0x44, 64, ..., 224) |
| Name: Port n Local ackID CSRs Offset: 0x48, 68, ..., 228 | | | |
| Bits | Name | Part | Section |
| 0 | Clr\_outstanding\_ackIDs | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.6 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 1:2 | Reserved | | |
| 3:7 | Inbound\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.6 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 8:18 | Reserved | | |
| 19:23 | Outstanding\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.6 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| 24:26 | Reserved | | |
| 27:31 | Outbound\_ackID | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.6 Port n Local ackID CSRs (Block Offsets 0x48, 68, ..., 228) |
| Name: Port n Error and Status CSRs Offset: 0x58, 78, ..., 238 | | | |
| Bits | Name | Part | Section |
| 0:4 | Reserved | | |
| 5 | Output Packet-dropped | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 6 | Output Failed-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 7 | Output Degraded-encountered | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offset 0x58, 78, ..., 238) |
| 8:10 | Reserved | | |
| 11 | Output Retry-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 12 | Output Retried | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 13 | Output Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 14 | Output Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 15 | Output Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 16:20 | Reserved | | |
| 21 | Input Retry-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 22 | Input Error-encountered | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 23 | Input Error-stopped | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 24:26 | Reserved | | |
| 27 | Port-write Pending | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 28 | Reserved | | |
| 29 | Port Error | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 30 | Port OK | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| 31 | Port Uninitialized | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.7 Port n Error and Status CSRs (Block Offset 0x58, 78, ..., 238) |
| Name: Port n Control CSR Offset: 0x5C, 7C, ..., 23C | | | |
| Bits | Name | Part | Section |
| 0:1 | Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 2:4 | Initialized Port Width | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 5:7 | Port Width Override | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 8 | Port Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 9 | Output Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 10 | Input Port Enable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 11 | Error Checking Disable | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 12 | Multicast-event Participant | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 13 | Flow Control Participant | RapidIO Interconnect Specification Part 9: Flow Control Logical Layer Extensions Specification | 4.3 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 14 | Enumeration Boundary | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 15:19 | Reserved | | |
| 20:27 | Re-transmit Suppression Mask | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |
| 28 | Stop on Port Failed-encountered Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 29 | Drop Packet Enable | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 30 | Port Lockout | RapidIO Interconnect Specification Part 8: Error Management Extensions Specification | 2.1 Additions to Existing Registers (Block Offsets 0x5C, 7C, ..., 23C) |
| 31 | Port Type | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.8.2.8 Port n Control CSR (Block Offsets 0x5C, 7C, ..., 23C) |

# Block: STD\_REG : Device Identity CAR

|  |  |  |  |
| --- | --- | --- | --- |
| Name: Device Identity CAR Offset: 0x00 | | | |
| Bits | Name | Part | Section |
| 0:15 | DeviceIdentity | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.1 Device Identity CAR (Configuration Space Offset 0x0) |
| 16:31 | DeviceVendorIdentity | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.1 Device Identity CAR (Configuration Space Offset 0x0) |
| Name: Device Information CAR Offset: 0x04 | | | |
| Bits | Name | Part | Section |
| 0:31 | DeviceRev | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.2 Device Information CAR (Configuration Space Offset 0x4) |
| Name: Assembly Identity CAR Offset: 0x08 | | | |
| Bits | Name | Part | Section |
| 0:15 | AssyIdentity | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.3 Assembly Identity CAR (Configuration Space Offset 0x8) |
| 16:31 | AssyVendorIdentity | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.3 Assembly Identity CAR (Configuration Space Offset 0x8) |
| Name: Assembly Information CAR Offset: 0x0C | | | |
| Bits | Name | Part | Section |
| 0:15 | AssyRev | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.4 Assembly Information CAR (Configuration Space Offset 0xC) |
| 16:31 | ExtendedFeaturesPtr | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.4 Assembly Information CAR (Configuration Space Offset 0xC) |
| Name: Processing Element Features CAR Offset: 0x10 | | | |
| Bits | Name | Part | Section |
| 0 | Bridge | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 1 | Memory | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 2 | Processor | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 3 | Switch | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 4:20 | Reserved | | |
| 21 | Multicast Support | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.2 Processing Elements Features CAR (Configuration Space Offset 0x10) |
| 22 | Extended route table configuration support | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.4.1 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 23 | Standard route table configuration support | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.4.1 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 24 | Flow Control Support | RapidIO Interconnect Specification Part 9: Flow Control Logical Layer Extensions Specification | 4.2 Processing Elements Features CAR (Configuration Space Offset 0x10) |
| 25 | Re-transmit Suppression Support | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.4.1 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 26 | CRF Support | RapidIO Interconnect Specification Part 6: 1x/4x LP-Serial Physical Layer Specification | 6.4.1 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 27 | Common transport large system support | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.4.1 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 28 | Extended features | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| 29:31 | Extended addressing support | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.5 Processing Element Features CAR (Configuration Space Offset 0x10) |
| Name: Switch Port Information CAR Offset: 0x14 | | | |
| Bits | Name | Part | Section |
| 0:15 | Reserved | | |
| 16:23 | PortTotal | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.6 Switch Port Information CAR (Configuration Space Offset 0x14) |
| 24:31 | PortNumber | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.6 Switch Port Information CAR (Configuration Space Offset 0x14) |
| Name: Source Operations CAR Offset: 0x18 | | | |
| Bits | Name | Part | Section |
| 0 | Read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 1 | Instruction read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 2 | Read-for-ownership | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 3 | Data cache invalidate | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 4 | Castout | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 5 | Data cache flush | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 6 | I/O read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 7 | Instruction cache invalidate | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 8 | TLB invalidate-entry | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 9 | TLB invalidate-entry sync | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 10:12 | Reserved | | |
| 13 | Data-streaming | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 14:15 | Implementation Defined | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 16 | Read | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 17 | Write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 18 | Streaming-write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 19 | Write-with-response | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 20 | Data message | RapidIO Interconnect Specification Part 2: Message Passing Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 21 | Doorbell | RapidIO Interconnect Specification Part 2: Message Passing Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| 22 | Atomic (compare-and-swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 23 | Atomic (test-and-swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 24 | Atomic (increment) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 25 | Atomic (decrement) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 26 | Atomic (set) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 27 | Atomic (clear) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 28 | Atomic (swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 29 | Port-write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.7 Source Operations CAR (Configuration Space Offset 0x18) |
| 30:31 | Implementation Defined | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.1 Source Operations CAR (Configuration Space Offset 0x18) |
| Name: Destination Operations CAR Offset: 0x1C | | | |
| Bits | Name | Part | Section |
| 0 | Read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 1 | Instruction read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 2 | Read-for-ownership | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 3 | Data cache invalidate | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 4 | Castout | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 5 | Data cache flush | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 6 | I/O read | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 7 | Instruction cache invalidate | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 8 | TLB invalidate-entry | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 9 | TLB invalidate-entry sync | RapidIO Interconnect Specification Part 5: Globally Shared Memory Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 10:12 | Reserved | | |
| 13 | Data-streaming | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 14:15 | Implementation Defined | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 16 | Read | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 17 | Write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 18 | Streaming-write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 19 | Write-with-response | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 20 | Data message | RapidIO Interconnect Specification Part 2: Message Passing Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 21 | Doorbell | RapidIO Interconnect Specification Part 2: Message Passing Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 22 | Atomic (compare-and-swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 23 | Atomic (test-and-swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 24 | Atomic (increment) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 25 | Atomic (decrement) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 26 | Atomic (set) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 27 | Atomic (clear) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 28 | Atomic (swap) | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 29 | Port-write | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.4.8 Destination Operations CAR (Configuration Space Offset 0x1C) |
| 30:31 | Implementation Defined | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.2 Destination Operations CAR (Configuration Space Offset 0x1C) |
| Name: Switch Multicast Support CAR Offset: 0x30 | | | |
| Bits | Name | Part | Section |
| 0 | Simple\_Assoc | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.3 Switch Multicast Support CAR (Configuration Space Offset 0x30) |
| 1:31 | Reserved | | |
| Name: Switch Route Table Destination ID Limit CAR Offset: 0x34 | | | |
| Bits | Name | Part | Section |
| 0:15 | Reserved | | |
| 16:31 | Max\_destID | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.4.2 Switch Route Table Destination ID Limit CAR (Configuration Space Offset 0x34) |
| Name: Switch Multicast Information CAR Offset: 0x38 | | | |
| Bits | Name | Part | Section |
| 0 | Block\_Assoc | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.4 Switch Multicast Information CAR (Configuration Space Offset 0x38) |
| 1 | Per\_Port\_Assoc | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.4 Switch Multicast Information CAR (Configuration Space Offset 0x38) |
| 2:15 | MaxDestIDAssoc | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.4 Switch Multicast Information CAR (Configuration Space Offset 0x38) |
| 16:31 | MaxMcastMasks | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.4 Switch Multicast Information CAR (Configuration Space Offset 0x38) |
| Name: Data Streaming Information CAR Offset: 0x3C | | | |
| Bits | Name | Part | Section |
| 0:15 | MaxPDU | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.3 Data Streaming Information CAR (Configuration Space Offset 0x3C) |
| 16:31 | SegSupport | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.4.3 Data Streaming Information CAR (Configuration Space Offset 0x3C) |
| Name: Data Streaming Logical Layer Control CSR Offset: 0x48 | | | |
| Bits | Name | Part | Section |
| 0:23 | Reserved | | |
| 24:31 | MTU | RapidIO Interconnect Specification Part 10: Data Streaming Logical Specification | 5.5.1 Data Streaming Logical Layer Control CSR (Configuration Space Offset 0x48) |
| Name: Processing Element Logical Layer Control CSR Offset: 0x4C | | | |
| Bits | Name | Part | Section |
| 0:28 | Reserved | | |
| 29:31 | Extended addressing control | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.5.1 Processing Element Logical Layer Control CSR (Configuration Space Offset 0x4C) |
| Name: Local Configuration Space Base Address 0 CSR Offset: 0x58 | | | |
| Bits | Name | Part | Section |
| 0 | Reserved | | |
| 1:16 | LCSBA | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.5.2 Local Configuration Space Base Address 0 CSR (Configuration Space Offset 0x58) |
| 17:31 | LCSBA | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.5.2 Local Configuration Space Base Address 0 CSR (Configuration Space Offset 0x58) |
| Name: Local Configuration Space Base Address 1 CSR Offset: 0x5C | | | |
| Bits | Name | Part | Section |
| 0 | LCSBA | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.5.3 Local Configuration Space Base Address 1 CSR (Configuration Space Offset 0x5C) |
| 1:31 | LCSBA | RapidIO Interconnect Specification Part 1: Input/Output Logical Specification | 5.5.3 Local Configuration Space Base Address 1 CSR (Configuration Space Offset 0x5C) |
| Name: Base Device ID CSR Offset: 0x60 | | | |
| Bits | Name | Part | Section |
| 0:7 | Reserved | | |
| 8:15 | Base\_deviceID | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.1 Base Device ID CSR (Configuration Space Offset 0x60) |
| 16:31 | Large\_base\_deviceID | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.1 Base Device ID CSR (Configuration Space Offset 0x60) |
| Name: Host Base Device ID Lock CSR Offset: 0x68 | | | |
| Bits | Name | Part | Section |
| 0:15 | Reserved | | |
| 16:31 | Host\_base\_deviceID | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.2 Host Base Device ID Lock CSR (Configuration Space Offset 0x68) |
| Name: Component Tag CSR Offset: 0x6C | | | |
| Bits | Name | Part | Section |
| 0:31 | component\_tag | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.3 Component Tag CSR (Configuration Space Offset 0x6C) |
| Name: Standard Route Configuration Destination ID Select CSR Offset: 0x70 | | | |
| Bits | Name | Part | Section |
| 0 | Ext\_config\_en | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.4 Standard Route Configuration Destination ID Select CSR (Configuration Space Offset 0x70) |
| 1:15 | Reserved | | |
| 16:23 | Config\_destID\_msb | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.4 Standard Route Configuration Destination ID Select CSR (Configuration Space Offset 0x70) |
| 24:31 | Config\_destID | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.4 Standard Route Configuration Destination ID Select CSR (Configuration Space Offset 0x70) |
| Name: Standard Route Configuration Port Select CSR Offset: 0x74 | | | |
| Bits | Name | Part | Section |
| 0:7 | Config\_output\_port3 | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.5 Standard Route Configuration Port Select CSR (Configuration Space Offset 0x74) |
| 8:15 | Config\_output\_port2 | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.5 Standard Route Configuration Port Select CSR (Configuration Space Offset 0x74) |
| 16:23 | Config\_output\_port1 | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.5 Standard Route Configuration Port Select CSR (Configuration Space Offset 0x74) |
| 24:31 | Config\_output\_port | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.5 Standard Route Configuration Port Select CSR (Configuration Space Offset 0x74) |
| Name: Standard Route Default Port CSR Offset: 0x78 | | | |
| Bits | Name | Part | Section |
| 0:23 | Reserved | | |
| 24:31 | Default\_output\_port | RapidIO Interconnect Specification Part 3: Common Transport Specification | 3.5.6 Standard Route Default Port CSR (Configuration Space Offset 0x78) |
| Name: Multicast Mask Port CSR Offset: 0x80 | | | |
| Bits | Name | Part | Section |
| 0:15 | Mcast\_Mask | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.5 Multicast Mask Port CSR (Configuration Space Offset 0x80) |
| 16:23 | Egress\_Port\_Num | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.5 Multicast Mask Port CSR (Configuration Space Offset 0x80) |
| 24 | Reserved | | |
| 25:27 | Mask\_Cmd | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.5 Multicast Mask Port CSR (Configuration Space Offset 0x80) |
| 28:30 | Reserved | | |
| 31 | Port\_Present | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.5 Multicast Mask Port CSR (Configuration Space Offset 0x80) |
| Name: Multicast Associate Select CSR Offset: 0x84 | | | |
| Bits | Name | Part | Section |
| 0:7 | Large\_DestID | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.6 Multicast Associate Select CSR (Configuration Space Offset 0x84) |
| 8:15 | DestID | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.6 Multicast Associate Select CSR (Configuration Space Offset 0x84) |
| 16:31 | Mcast\_Mask\_Num | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.6 Multicast Associate Select CSR (Configuration Space Offset 0x84) |
| Name: Multicast Associate Operation CSR Offset: 0x88 | | | |
| Bits | Name | Part | Section |
| 0:15 | Assoc\_Blksize | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |
| 16:23 | Ingress\_Port | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |
| 24 | Large\_Transport | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |
| 25:26 | Assoc\_Cmd | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |
| 27:30 | - | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |
| 31 | Assoc\_Present | RapidIO Interconnect Specification Part 11: Multicast Extensions Specification | 3.7 Multicast Associate Operation CSR (Configuration Space Offset 0x88) |